Overview
--:--:--
⚠ 3 Active Faults
CPU 315-2 DP
Main Winch Load
187T
▲ 62% of rated
Hoist Speed
12.4m/min
● Lowering
Slew Angle
47.2°
→ Port side
Luff Angle
62.8°
⚠ Near upper limit
Main Winch Load — Last 30 min
Drive Status — All Axes
🤖
AI Assistant
ZPMC Crane Expert · Claude Sonnet
AI ASSISTANT
Halo! Saya AI specialist ZPMC ZP11-175 (powered by Groq · LLaMA 3.3 70B). Saya siap membantu troubleshoot, diagnosa fault, commissioning, dan parameter drives crane ini. Default backend: cPanel (aman, tanpa perlu input API key). Kalau mau ganti mode, klik tombol [⚙ Backend] di kanan atas. How can I help?
Main Winch
Aux Winch
Luff
Slew
Absolute Encoders — P+F Multiturn
Position Trend
⚙ Encoder specs: Pepperl+Fuchs V2.2 Multiturn, SSI interface, PROFIBUS DP address 256–297
All encoders connected via ET200 distributed I/O on PROFIBUS DP master (CPU 315-2)
Encoder Health Diagnostics

Encoder | Address | Resolution | Position | Status | Last Update
--- | --- | --- | --- | --- | ---

Dual-Engine Synchronization & Interlocks
Engine Speed Trend — Last 30 min
AI Engine Diagnostics
Lubricant Oil Filter
Cooling System — Water & Fans
Oil Return / Jam Signals (FS1–FS4)
Pressure Sensor Network — B1 to B16 (crane running permit requires ≥ 20.0 bar)

Sensor | Function | S7 Address Code | Pressure (bar) | Threshold | Status
--- | --- | --- | --- | --- | ---

AI Hydraulic Power Pack Diagnostics
Active Faults
3
Warnings
4
Today Total
13
Active Alarms & Fault Log
AI Fault Analysis
DP Master
CPU 315-2 DP — ONLINE
Baud: 1.5 Mbit/s · HSA: 126
DP Slaves Active
12 / 13
● 1 slave offline
PROFIBUS DP Node Map — ZP11-175
Network Diagnostics
Drive Params
PLC Config
Safety Limits
from S7 hardware config

Parameter | Value | Range / Type | Status
--- | --- | --- | ---

🤖
ZPMC Crane AI Specialist
Powered by Claude Sonnet · Expert in ZPMC Big Crane, Siemens S7, PROFIBUS, VFD drives