OFFSHORE AI ⛴️ diagnostic
AI 24/7 Offshore

# REDUCE OFFSHORE
EQUIPMENT DOWNTIME WITH AI

Analyze mooring winches, cranes, tensioners, hydraulic systems and offshore equipment in minutes instead of hours. Faster troubleshooting. Less downtime. Better decisions.

AI Diagnostics 24/7 Support Offshore Focus
AI DIAGNOSTIC live
FAULT CODE
SL1 Trip
HEALTH SCORE
72%
ROOT CAUSE
Encoder signal loss
RECOMMEND
Check feedback
⚡ Fault analysis 🔍 Root cause 📋 Maintenance plan

## LIVE PRODUCTS

Production-ready AI assistants for offshore operations.

LIVE

### Mooring Winch AI

Analyze Unidrive SP, fault codes, CTSoft exports.

LIVE

### Crane Diagnostic AI

Troubleshooting for offshore and port cranes.

LIVE

### Clyde 37-DE · RCI-1550

Robway RCI-1550 Rated Capacity Indicator diagnostic & calibration.

Load Cell Cal ATB Motion Cut
IN DEVELOPMENT

### Engine Room Copilot

Generator, propulsion & auxiliary diagnostics — Coming Q4 2026

Currently in active development
IN DEVELOPMENT

### Maintenance Assistant

Planning and troubleshooting recommendations — Coming Q1 2027

Beta program opening soon
IN DEVELOPMENT

### ICT Solutions

VSAT, Starlink, Mikrotik, Firewall, Network optimization — Coming Q3 2026

Infrastructure design in progress

## WHY OFFSHORE TEAMS CHOOSE OFFSHOREAI

80%
Faster Troubleshooting
70%
Reduced Diagnostic Time
24/7
AI Technical Assistance
100%
Standardized Analysis

## BUILT FOR REAL OFFSHORE OPERATIONS

Developed using practical experience from marine and offshore environments.

### Marine Engineering

Designed around real vessel equipment.

### Offshore Operations

Built for offshore maintenance challenges.

### Electrical Systems

Drives, motors, controls & diagnostics.

### Maritime Comms

VSAT, Starlink & vessel connectivity.

## AI TOOLS BUILT FOR OFFSHORE

### Mooring Winch AI

- ✓ Unidrive SP Analysis
- ✓ CTSoft Parameter Review
- ✓ Trip Analysis
- ✓ Root Cause Detection

### Crane Diagnostic AI

- ✓ Hoist Systems
- ✓ Slewing Systems
- ✓ Hydraulic Analysis
- ✓ Electrical Diagnostics

### Clyde 37-DE · RCI-1550

- ✓ Load Cell Calibration (F-02, F-03)
- ✓ Boom Angle & Length (F-08, F-09)
- ✓ ATB / Over-hoist (Error 220)
- ✓ CPU Box Troubleshooting

## REAL DIAGNOSTIC EXAMPLE

See how OffshoreAI accelerates troubleshooting.

### INPUT

Equipment Mooring Winch
Drive Unidrive SP
Fault SL1 Trip
Action Upload fault details
AI OUTPUT
Root Cause:
Encoder Signal Loss
Recommended Actions:

- ✓ Verify encoder cable
- ✓ Check feedback module
- ✓ Confirm power supply
- ✓ Test encoder output

Result: Time reduced from hours to minutes.

## WHY TRUST OFFSHOREAI?

### Real Offshore Experience

Working with offshore equipment and vessel systems.

### Field-Based Diagnostics

Built around real fault cases and workflows.

### Industry-Specific AI

Not a generic chatbot. Purpose-built for marine & offshore.

### Continuous Improvement

Models enhanced using operational feedback.

## ENTERPRISE SOLUTIONS

Custom AI for your vessel, equipment, or engineering team.

### Custom Vessel AI

Tailored AI for vessel operations.

### Custom Equipment AI

Dedicated diagnostic assistant.

### Company Knowledge AI

AI trained on manuals & procedures.

## READY TO REDUCE OFFSHORE DOWNTIME?

Start with our live Mooring Winch AI or schedule a consultation.

🔒

## Trial Expired

You've reached the limit of your free trial. Unlock full access to continue.

Remaining: 0 tries
$99 /month

No commitment. Cancel anytime.

OffshoreAI Assistant
EN · ID · OFFSHORE · DIAGNOSTIC
Online
⛴️ Powered by OffshoreAI Knowledge Base · EN/ID