Overview
--:--:--
⚠ 2 Active 📡 cPanel
Load Trend — Last 30 min RCI-1550
RCI-1550 LED Indicators
Override
Alarm Disabled
ATB
Approach 85%
100% Exceeded
Motion Cut
⚠ Motion Cut Active · ATB Detected
🤖 AI Assistant Multi-Language
🤖 AI Technician ready. Ask about errors, calibration, or troubleshooting.
💡 Examples: "Error 220", "How to calibrate load cell", "CPU Box troubleshooting"
📡 RCI-1550 Sensor Detail Live
Load (Main)45.2 T
Load (Aux)0.0 T
Boom Angle 82.0°
Boom Length 48.8 m
Radius 15.2 m
Height 56.3 m
SWL 250 Ton
% SWL 19%
0%85%100%
✓ SWL: 19% · Safe
🏗️ Clyde 37-DE Specs CW-3936
SWL (Revolving)250 Ton (276 S.Ton)
SWL Aux. Hook 30 Ton (33 S.Ton)
SWL Whip Hook 10 Ton (11 S.Ton)
Max Reach 64 m (210 ft)
Max Height 64 m (210 ft)
Main Engine Cat D-3406
Hoist Engine Cat D-346
Swing Engine Cat D-343 (DC)
Tensiometer RW5000 Load Cell
Active Faults
2
Warnings
1
Motion Cut
Active
RCI-1550 Error Log Active

Code | Description | Status
--- | --- | ---
220 | ATB / Over-hoist | Active
240 | Overload 100% SWL | Pending
— | No other errors | Clear

🔍 AI Fault Analysis
🤖 Click button below for error analysis.
🎮 Control & Override RCI-1550
Rigging Mode
Off
Temp ATB Override
Off
Mute Alarm
Falls Main: 8 Falls Aux: 2 Duty: 24 Winch: #1 Main
⚙️ Quick F-Code Calibration
📋 RCI-1550 Function Codes (F-Code) Reference
🤖 RCI-1550 AI Specialist Multi-Language
🤖 AI Specialist ready. Ask anything about RCI-1550, calibration, troubleshooting, or Clyde 37-DE.
💡 Ask in English or Indonesian — answer will match your language.